Set Reset flip-flop schematic



